Vinotéka Guzzanti GZ 52A

Prosklená vinotéka s kompresorem

* kapacita 52 láhví vína, 133l
* stabilní chlazení díky kompresoru a  eko chladivu R600a
* černé dveře s nerezovou rukojetí
* 3+1 dřevěné police
* max. hlučnost do 39dB
* elektronická  kontrola LED  display +  digitální termostat s regulací po 1C
* vnitřní LED osvětlení
* dvířka ze zakřiveného dvouvrstvého temperovaného skla, které chrání víno před slunečním zářením a světlem
* chladicí rozsah 5 - 22°C
* spotřeba energie 0,40 kWh/24h, energetická třída A
* ideální pro hotely, penziony, kanceláře

Model GZ 52A  
EAN 8594186721030  
Rozměry (V x Š x H) 82,5 x 52,5 x 63,2 cm  
Váha 36 kg  
Rozměry balení (V x Š x H) 84,5 x 57,5 x 60,7 cm  
Váha balení 39 kg  
Barva černá, černý interiér  
  
  
Winecooler Guzzanti GZ 52A  
  
Glass door winecooler with compressor

* volume 52 bottles, 133l
* 3 + 1 wooden racks
* noise level – up to 39dB
* electronic control LED display + digital thermostat with 1°C regulation
* cooling range 5 - 22°C
* inner LED light
* door made of curved, tempered and hardened two ply glass protecting wine from sunlight and light
* black door with stainless steel handle
* suitable for hotels, bed&breakfasts, restaurants, offices
* power consumption 0,40 kWh/24 h, energy class A
* stable compressor cooling with R600a eco refrigerant

Model GZ 52A  
EAN 8594186721030  
Dimensions (H x W x D) 82,5 x 52,5 x 63,2 cm  
Weight 36 kg  
Packing dims. (H x W x D) 84,5 x 57,5 x 60,7 cm  
Packing weight 39 kg  
Color black, black interior